CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Sat Apr 15 12:11:37 2023
Release      : TopSpin 4.1.3
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.1.166.20220113
CPU          : Intel(R) Core(TM) i5-8400H CPU @ 2.50GHz (8 cores at 3907 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 750 NMR spectrometer
1H-frequency : 750.30 MHz
Description  : Avance NEO
Bruker Order : 442759
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- SCU: AV4I SCU SYSTEM CONTROL UNIT Z162978/00387 ECL 02.00
- {EPU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00387 ECL 02.00
- {GTU}: AV4I SCU SYSTEM CONTROL UNIT Z162978/00387 ECL 02.00
  Location: slot 7 in rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20210312125813
  - Gradient resolution: 1.0 us
  Devices: MTD at /dev/mtd2, RTD at /dev/bbu/rtd4.4, GPROC at /dev/bbu/gproc4.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06699 ECL 02.05
  Location: slot 3 in rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd11, DRX at /dev/bbu/drx9.5, RTD at /dev/bbu/rtd9.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06698 ECL 02.05
  Location: slot 4 in rack 1
  Connection: at IP 192.168.180.46 via PCIe #11
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd20, DRX at /dev/bbu/drx11.5, RTD at /dev/bbu/rtd11.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/06700 ECL 02.05
  Location: slot 5 in rack 1
  Connection: at IP 192.168.180.54 via PCIe #13
  Firmware Version: 20210312121750
  Devices: MTD at /dev/mtd29, DRX at /dev/bbu/drx13.5, RTD at /dev/bbu/rtd13.4
  Sequencer: FCube
  - FCube3
- PSM-A: AV4 PSM-A Z149510/02732 ECL 03.01
- HPPR/2 COVER2: HPPR/2 Cover2N Z178831/00167 ECL 00.00
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 1H19F (reflection meter with CRP-Bias capability)
                  PN=Z103207, SN=00209 from 20210618
      Module  2 : 2H
                  PN=Z003475, SN=00210 from 20190312
      Module  3 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111095, SN=00223 from 20190705
      Module  4 : 13C/79Br
                  PN=Z003526, SN=00207 from 20180612
      Module  5 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111095, SN=00221 from 20190315
      Module  6 : 31P
                  PN=Z102451, SN=00200 from 20210622
  
- HPLNA 1H19F: HPLNA 1H MODULE 750 Z103207/00209 ECL 06.05
- 2H: HPPR/2 2H MODULE 750 Z003475/00210 ECL 07.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 750 Z111095/00223 ECL 04.04
- 13C/79Br: HPPR/2 13C MODULE 750 Z003526/00207 ECL 08.00
- HPLNA BB31P: HPLNA XBB 31P MODULE 750 Z111095/00221 ECL 04.04
- 31P: HPPR/2 31P MODULE 750 Z102451/00200 ECL 07.01
- RACK: AV4I AQS CHASSIS Z175600/00370 ECL 00.00
- PSM-48V: AV4 PSM-48V Z149850/04474 ECL 01.02
- PSM-D: AV4 PSM-D Z149520/02583 ECL 01.01
- FANTRAY: AV4I AQS FAN TRAY Z175900/00312 ECL 00.00
- REF 1200: AV4 REFERENCE 1200 Z148270/02367 ECL 02.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144060-000236 W144060/000236 ECL 41:
- TCP/IP address = 192.168.99.13
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB1000 15-600: W144060/000236 ECL 41
- Controller     = BLA CONTROL BOARD 7: W133936/025326 ECL 40
BLA-W144060-000235 W144060/000235 ECL 41:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20210223
- Amplifier      = AV4 BLABB1000 15-600: W144060/000235 ECL 41
- Controller     = BLA CONTROL BOARD 7: W133936/025302 ECL 40
BLA-W144058-000036 W144058/000036 ECL 02:
- TCP/IP address = 192.168.99.11
- Firmware VS    = 20210223
- Amplifier      = AV4 BLAH1000 700-900: W144058/000036 ECL 02
- Controller     = BLA CONTROL BOARD 7: W133936/023492 ECL 40
LTRX Z109892/00208 ECL 02.02:
- TCP/IP address = 192.168.99.10
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 750: Z109892/00208 ECL 02.02

Gradient amplifiers at the spectrometer subnet:
----------------------------------------------
BGA1: BGAU_W154248_0136
- TCP/IP address   = 192.168.99.16
- Firmware version = 20210916
- Web version      = 8.10
- Current limits   = 0.0/X, 0.0/Y, 0.0/Z (in A)
BGA2: BGAU_W154248_0137
- TCP/IP address   = 192.168.99.15
- Firmware version = 20210916
- Web version      = 8.10
- Current limits   = 0.0/X, 0.0/Y, 0.0/Z (in A)
BGA3: BGAU_W154248_0139
- TCP/IP address   = 192.168.99.14
- Firmware version = 20210916
- Web version      = 8.10
- Current limits   = 0.0/X, 0.0/Y, 0.0/Z (in A)

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10
- ELCB firmware version = 20210921
- ELCB = BSMS/2 ELCB: Z100818/09250 ECL 07.03
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- Shim System = BOSS-WB
- SCB channels = 40
- Shim matrix file: 272623fa.dat
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z2 XZ4 XZ3 Z6 (X2-Y2)Z YZ4 YZ3 XYZ2 XYZ X3Z X3 Y3Z Y3 (X2-Y2)Z3 XYZ3
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- L-TRX = BSMS/2 LOCK TRANSCEIVER 750: Z109892/00208 ECL 02.02
- Lock: on L-TRX board, supports 2H
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00870 ECL 05.05
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC-E: Z140144/00301 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.10

- Firmware version = 20220315_1040
MAS Control Unit: MAS_H139288_0479
- TCP/IP address   = 192.168.98.5

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101
Line Distribution Unit 3: PDU3
- TCP/IP address   = 192.168.99.102


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 3 (AV4 BLAH1000 700-900 W144058/000036 at TCP/IP 192.168.99.11)
TRX1 AUX  output -> input 1 of transmitter 4 (BSMS/2 LOCK TRANSCEIVER 750 Z109892/00208 at TCP/IP 192.168.99.10)
TRX2 NORM output -> input 1 of transmitter 2 (AV4 BLABB1000 15-600 W144060/000235 at TCP/IP 192.168.99.12)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 1 (AV4 BLABB1000 15-600 W144060/000236 at TCP/IP 192.168.99.13)
TRX3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB1000 15-600 W144060/000236 at TCP/IP 192.168.99.13:
- amplifier B-1000W uses blanking 3
- amplifier B-100W uses blanking 3

transmitter 2 = AV4 BLABB1000 15-600 W144060/000235 at TCP/IP 192.168.99.12:
- amplifier B-1000W uses blanking 2
- amplifier B-100W uses blanking 2

transmitter 3 = AV4 BLAH1000 700-900 W144058/000036 at TCP/IP 192.168.99.11:
- amplifier 1H-1000W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 750 Z109892/00208 at TCP/IP 192.168.99.10:
- amplifier 2H-5W uses blanking 9


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 1H19F -> REC1
Tune-TRX1 -> 2H          -> REC1
Tune-TRX2 -> HPLNA BB31P -> REC2
Tune-TRX2 -> 13C/79Br    -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3
Tune-TRX3 -> 31P         -> REC3

